QGIS procedures to make zonal values and statistics

1. select layer that want to proceed, e.g. 400mm, 500 mm etc.

2. clip ‘Harvey imapct’ vector by that layer

…